**Simulation Report 2**

Yifu Huang

**Codes for data processing:**

<https://github.com/yifuhhh/EE396V_TFT/blob/master/DataProcess/Project_2.py>

**Script for one of the bulk trap sweeps:**

<https://github.com/yifuhhh/EE396V_TFT/blob/master/Prj_2/prg_2_bulkshallow/TFT_bulkshallow.in>

**Script for channel length sweep:**

<https://github.com/yifuhhh/EE396V_TFT/blob/master/Prj_2/prg_4_channel/TFT_channel.in>

**Section I**

1. **Interface trap peak density**

地图的截图

描述已自动生成

Figure 1.1 Trap density of states for sweep of interface trap

手机屏幕截图

描述已自动生成

Figure 1.2 Transfer curve for sweep of interface trap, linear scale

地图的截图

描述已自动生成

Figure 1.3 Transfer curve for sweep of interface trap, log scale

From Fig 1.2 and 1.3, it is observed that when the density of acceptor-like states in the tail distribution at the conduction band edge in interface increases, Id would decrease at the same Vgs.

地图的截图

描述已自动生成

Figure 1.4 Threshold voltage for sweep of interface trap

From Figure 1.4, it is observed that Vth increases as the density of acceptor-like states in the tail distribution at the conduction band edge in interface increases.

手机屏幕的截图

描述已自动生成

Figure 1.5 Subthreshold swing for sweep of interface trap

From Figure 1.5, it is observed that subthreshold swing decreases as the density of acceptor-like states in the tail distribution at the conduction band edge in interface increases.

1. **Bulk shallow trap peak density**

地图的截图

描述已自动生成

Figure 2.1 Trap density of states for sweep of bulk shallow trap

手机屏幕截图

描述已自动生成

Figure 2.2 Transfer curve for sweep of bulk shallow trap, linear scale

地图的截图

描述已自动生成

Figure 2.3 Transfer curve for sweep of bulk shallow trap, log scale

From Fig 2.2 and 2.3, it is observed that when the density of acceptor-like and donor-like states in the tail distribution at the conduction band edge in shallow bulk increases, Id would decrease at the same Vgs when Vgs > 0.

手机屏幕截图

描述已自动生成

Figure 2.4 Threshold voltage for sweep of bulk shallow trap

From Figure 2.4, it is observed that Vth gets maximum at NTA & NTD = 2e21 cm-3/eV. However, it is not consistent with the trend in Figure 2.2. The main reason for this phenomenon is that in our simulation, Vgs goes up to 20 V. To fully describe the transfer performance especially when NTA & NTD = 8e21 cm-3/eV, Vgs has to increase more.

地图的截图

描述已自动生成

Figure 2.5 Subthreshold swing for sweep of bulk shallow trap

From Figure 2.5, it is observed that subthreshold swing (absolute value) gets minimum at NTA & NTD = 2e21 cm-3/eV.

1. **Bulk deep trap peak density**

手机屏幕截图

描述已自动生成

Figure 3.1 Trap density of states for sweep of bulk deep trap

手机屏幕截图

描述已自动生成

Figure 3.2 Transfer curve for sweep of bulk deep trap, linear scale

地图的截图

描述已自动生成

Figure 3.3 Transfer curve for sweep of bulk deep trap, log scale

From Fig 3.2 and 3.3, it is observed that when total density of donor-like states in a Gaussian distribution in the deep bulk increases, Id would not be affected a lot when Vgs > 0 and Id would decrease as NGD increases when Vgs < 0.

地图的截图

描述已自动生成

Figure 3.4 Threshold voltage for sweep of bulk deep trap

From Figure 3.4, it is observed that Vth decreases as NGD increases.

地图的截图

描述已自动生成

Figure 3.5 Subthreshold swing for sweep of bulk deep trap

From Figure 3.5, it is observed that subthreshold swing (absolute value) gets minimum at NGD = 2e16 cm-3/eV.

**Section II**

1. Channel length

手机屏幕截图

描述已自动生成

Figure 4.1 Transfer curve for sweep of channel length, linear scale

地图的截图

描述已自动生成

Figure 4.2 Transfer curve for sweep of channel length, log scale

From Fig 4.1 and 4.2, it is observed that when channel length increases, Id would decrease at the same Vgs > 0.

手机屏幕截图

描述已自动生成

Figure 4.3 Threshold voltage for sweep of channel length

From Figure 4.3, it is observed that Vth increases as channel length increases.

手机屏幕截图

描述已自动生成

Figure 4.4 Subthreshold swing for sweep of channel length

From Figure 4.4, it is observed that subthreshold swing (absolute value) gets minimum at channel length = 30 um.